SMU - SECTION 0B - INCORRECT LISTING OF ENGINE FUEL FILTERS. Buick Coachbuilder 1990

For 1990-2009 cars

# SMU - SECTION 0B - INCORRECT LISTING OF ENGINE FUEL FILTERS

---------------------------------------------------------------------- SERVICE MANUAL UPDATE ----------------------------------------------------------------------

#### SUBJECT: SECTION 0B - INCORRECT LISTING OF ENGINE FUEL FILTER

#### MODELS: 1990 BUICK ESTATE WAGON 1990 CHEVROLET CAPRICE 1990 OLDSMOBILE CUSTOM CRUISER WAGON

THE 1990 B-CARLINE SERVICE MANUAL INCORRECTLY LISTS THE REPLACEMENT FUEL FILTERS IN SECTION 0B, PAGE 8. THE CORRECT FUEL FILTER REPLACEMENT P/N'S ARE AS FOLLOWS:

ENGINE A/C TYPE GM P/N

4.3L (VIN Z) GF 580 25121468 5.0L (VIN E) GF 580 25121468 5.0L (VIN 7) GF 580 25121468 5.0L (VIN Y) GF 471 05651803

#### PART AVAILABILITY:

PARTS ARE CURRENTLY AVAILABLE FROM GMSPO.

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.