WATER LEAK IN TRUNK AREA INSTALL CAULK MOUNTING STUDS. Buick Coachbuilder 1992

For 1990-2009 cars

# WATER LEAK IN TRUNK AREA INSTALL CAULK MOUNTING STUDS

#### SUBJECT: WATER LEAK IN TRUNK AREA (INSTALL STRIP CAULK AROUND BEZEL MOUNTING STUDS)

#### VEHICLES AFFECTED: 1992 "B" MODEL

#### APPLICATION:

Buick Roadmaster "B" Model (prior to VIN 1G4BN532NR472540).

#### CONDITION:

Water leak in trunk area.

#### CAUSE:

May be due to missing washers on opera lamp bezel mounted in sail panel area. See Service Manual, Section 8B or 10-9.

#### CORRECTION:

Remove bezel and opera lamp and install strip caulk around the bezel mounting studs in place of the missing washers and re-install bezel to vehicle.

See Service Manual, Section 8B or 10-9 for opera lamp location and instructions for removal and reinstallation.

For vehicles repaired under warranty use:

Labour Operation: N1190 Right Side N1191 Left Side

Labour Time: 0.2 Hr. 0.2 Hr.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.