PAINT INFORMATION. Buick Coachbuilder 1994

For 1990-2009 cars

# PAINT INFORMATION

#### SUBJECT: PAINT INFORMATION

#### MODELS: 1994 BUICK PRODUCTS

THE FOLLOWING CHART PROVIDES PAINT INFORMATION ON 1994 BUICK PRODUCTS. THE PAINT TYPES LISTED BELOW THE MODELS INDICATE THE MATERIAL THE VEHICLE WAS MANUFACTURED WITH. MODELS PAINT TYPE CODE# NAME WA# A B C H N W BASF DUP * PPG DUP DUP

08 MARY KAY PINK 9601 13 SILVER MET. 9021 X X 14 LT. GRAY MET. 9789 X X X X X 16 BRIGHT WHITE 9753 X X X X X X 18 DK. GREEN GRAY MET. 9795 X X X X 23 LT. CLOISONNE MET. 126A X 26 MED. CLOISONNE MET. 127A X 30 MED. ADRIATIC MET. 9907 X X X X X X 33 LT. DRIFTWOOD MET. 5322 X X X X 36 LT. ADRIATIC MET. 121A X X 36 LT. ADRIATIC MET. 173A X X 39 DK. ADRIATIC MET. 122A X 41 BLACK 8555 X X X X X X 43 BRIGHT AQUA MET. 9796 X 44 MED. MALACHITE MET. 9084 X 45 MED. GREEN PEARL 9539 X 48 DK. YELLOW GRN. MET. 9806 X X 57 LT. BEIGE MET. 9805 X X 72 MED. GARNET RED MET. 8979 X X X X X X 76 DK. GARNET RED MET. 8984 X 77 DK. CHERRY MET. 9800 X X X X 81 BRIGHT RED 8774 X 91 PURPLE PEARL 9926 X X X X X

PAINT TYPES: DUP= DUPONT, PPG= PPG, BASF= BASF

* "C" MODELS BUILT IN WENTZVILLE (PLANT CODE 1) USE BASF BUILT IN BUICK CITY (PLANT CODE H) USE PPG

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1993 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.