GM GOODWRENCH 350 DIESEL ENGINE P/N'S. Buick Electra Estate Wagon 1981

For 1990-2009 cars

# GM GOODWRENCH 350 DIESEL ENGINE P/N'S

A GM Goodwrench 350 diesel engine is now available through WDDGM for certain current and past model vehicles equipped with a 5.7 liter V8 diesel engine. All GM Goodwrench 350 diesel engines are manufactured with new components. They all contain roller lifter valve trains and incorporate all parts, except as noted below:

APPLICATION - GM-GOODWRENCH 350 DIESEL ENGINE

Engine Part Number 22520957 22523103 22522089 (I.D. Code MG1) (I.D.Code MG2) (I.D.Code MG3)

Passenger Car

Oldsmobile, 1978-79 1980 ALL 1981 Except Buick, Cadillac, 1981 California California Chevrolet, and 1982-83 ALL Pontiac

Light Duty Truck

Chevrolet and 1978-79-80 1981 California GMC

#### NOTICE: 1981 model Canadian and export passenger cars and 1981 model light duty trucks built with pencil type nozzles and internal EGR cylinder heads cannot utilize a GM Goodwrench 350 diesel engine. It will be necessary to utilize a partial engine or fitted block currently available from WDDGM.

Description

1. Engine 22520957 (Code MG1) contains cylinder heads machined for PENCIL type nozzles. There are no provisions for EGR.

2. Engine 22523103 (Code MG2) contains cylinder heads machined for POPPET type nozzles. These cylinder heads are manufactured to match intake manifolds with EXTERNAL EGR.

3. Engine 22522089 (Code MG3) contains cylinder heads machined for POPPET type nozzles. These cylinder heads are manufactured to match intake manifolds with INTERNAL EGR.

What's Included

Cylinder block assembly, connecting rod and piston assemblies, crankshaft, crankshaft balancer, camshaft, cylinder head assemblies including valve trains, camshaft and crankshaft sprockets with chain, timing gears and timing cover, oil pump and screen, oil pan and installation instruction sheet.

Ordering Information

GM Goodwrench Diesels can be ordered to meet your needs and those of your customers.

If a customer's car is down and a replacement unit is needed, get fast delivery by ordering through the RAPID system, V.I.P. or C.I.O. classifications, or by calling direct to your local Parts Distribution Center.

Stock orders can be placed using either Supplemental or Regular stock order classifications. For either stock or V.I.P./C.I.O. classifications, normal pricing policies will apply. Should you want to serve as a supplementary source of supply in your area, or if you want to take advantage of significant discounts and allowances, order using a green "Direct Ship" order form. We've reproduced an example below. You can save a minimum of $84 per unit, plus 8% parts return reserve and 3% advertising assistance allowance, by ordering the truckload quantity.

(NOTE: Only truckload quantities may be ordered on that form.)

If you have any questions, or need more information, please consult your GM Parts Sales District Manager.

The New GM Goodwrench 350 Diesel Engine Packages

These new GM Goodwrench replacement engines have been designed to appeal to both Buick/Dealers and their customers. Check out these benefits:

12 Month/12,000 Mile Limited Warranty provides desired protection for the consumer,

Cost Advantages: The $1,200 dealer net price (plus labor) for the GM Goodwrench Diesels will save your customers approximately $925.00 over the cost of using a Partial Engine, and the additional parts and labor required for rebuilding.

Dealer Installation Benefits: These replacement engines are calculated to provide for an efficient and productive use of service personnel, generating income for the dealership while offering prompt satisfaction for the customer. The applications for the GM Goodwrench 350 Diesel engines are illustrated in the chart below.

PASSENGER VEHICLE AND LIGHT-DUTY TRUCK APPLICATION

DESCRIPTION AND USAGE OF GM GOODWRENCH 5.7 LITER 350 DIESEL ENGINE

5.7 LITER (350 CID) Diesel Engine All engines utilize current model blocks, crankshaft, and roller lifter valve trains.

Passenger Car 22520957 22523103 22522089 Application Engine #1 Engine #2 Engine #3

Oldsmobile, Buick, 1978-79 1980 ALL 1981 Except Cadillac, Chevrolet, 1981 Califomia California and Pontiac 1982-83 ALL

*Light-Duty Truck 1978-79-80 1981 California Application Engine #1 Engine #2 Engine #3 Pencil nozzle Poppet nozzle Poppet nozzle No EGR External EGR Internal EGR 16 Distribution 5 Distribution 8 Distribution Centers Centers Centers

*Not available for 1981 Federal Light-Duty Trucks.

WHAT'S INCLUDED:

Cylinder block assembly Connecting rod and piston assemblies Crankshaft Crankshaft balancer Camshaft Cylinder head assemblies, including valve trains Camshaft and camshaft sprockets with chain Timing gears and timing cover Oil pump and screen Oil pan Installation instructlon sheet

WHAT'S NOT INCLUDED:

Most often you can transfer these from the engine that is being replaced. These parts are: The intake manifold and related plumbing Exhaust manifolds Alternator Power steering Vacuum pump Injection pump Injection nozzles and pipes Fuel pump Filter and pipes Water pump Flywheel Pulleys Brackets and belts

What's Not Included

Most often you can transfer these from the engine that is being replaced. These parts are: the intake manifold and related plumbing, exhaust manifolds, alternator, power steering, vacuum pump, injection pump, injection nozzles and pipes, fuel pump, filter and pipes, water pump, block heater, flywheel, pulleys, brackets and belts.

What Must Be Ordered Separately

Guide - Oil Level Indicator

Gasket Kit - Intake Manifold

Gasket - Water Pump Body

Gasket - Oil Filter Base

Gasket - Fuel Pump

Seal - Injection Nozzle Carbon Stop. (8) Required (Pencil Type Nozzle Only)

Seal - Injection Nozzle Compression. (8) Required (Pencil Type Nozzle Only)

Spacer - Nozzle spring clamp #22505830 (Pencil Type Nozzle Only-See Note)

Clamp Assembly - Fuel Injection Nozzle #22505829 (Pencil Type Nozzle Only-See Note)

Seal - Vacuum Pump "O" Ring

Pump Assembly - Vacuum #7839413 (Required only on 1978 Models Unless Camshaft Package #22502676 has Previously Been Installed)

Gasket - Oil Pan Package Required on All Riviera Models Only

#### NOTE: Second design nozzle spacers and clamps will be required unless a cylinder head has previously been replaced. The second design clamp uses a 3/8" bolt, the first design was 5/16". Remove one bolt from each cylinder head to determine which style is installed on the engine. Order separately as required.

Service Parts

The GM Goodwrench 350 diesel engine uses current model parts, except as listed on the following chart. When servicing a vehicle with 5.7 liter diesel engine, it will be necessary to determine if a GM Goodwrench 350 diesel engine has been installed. Each GM Goodwrench 350 diesel engine will have a distinctive label on each valve cover for easy identification. In addition, you will be supplied an additional label to attach to the front of the air cleaner. These visual aids will allow you to readily identify this engine and order the proper parts for service.

SERVICE REPAIR

For service repair, the following part numbers are specific:

Engine Number 22520957 22523103 22522089

Cylinder Heads 22523637 22523638 1983 Model (Refer to Parts Catalog for Part Number)

Pistons 1978 Through 1978 Through 1983 Model 1981 Models 1981 Models (Refer to Parts (Refer to Parts (Refer to Parts Catalog for Catalog for Catalog for Part Number) Part Number) Part Number)

All other parts contained in the GM-Goodwrench 350 diesel engine are 1983 model parts and should be ordered from the current 1983 Parts Catalog.

Warranty Information

Any warranty claims submitted to Buick for the installation of a GM Goodwrench 350 diesel engine will require zone authorization, and are to be submitted using the following labor operation number. List the applicable engine part number in the "Failed Part Number" column.

Labor Time Allowance:

Riviera All Others

1980-81-82-83 Models J1840 8.4 7.7

#### Add:

With cruise control .1 hr. With A/c .5 hr. Replace govenor weight retainer ring (if required) .7 hr.

Includes: R&R hood, belts, fan and flywheel cover. D&C exhaust pipes, fuel and vacuum lines, linkage, starter and hoses. Drain and refill engine oil (if required) and coolant. Transfer oil pan and pump on Riviera. Check injection pump governor weight retainer ring. Make all necessary adjustments including timing. Also includes time to transfer all required parts.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.