ENGINE OIL PAN GASKETS STEEL CORE WITH BONDED CORK. Buick Electra Estate Wagon 1983

For 1990-2009 cars

# ENGINE OIL PAN GASKETS STEEL CORE WITH BONDED CORK

#### MODELS AFFECTED: 1983 5.0 V-8 (VIN CODE Y) GAS, 4.3L V-6 AND 5.7L V-8 DIESEL ENGINES

The oil pan gasket on the engines listed above contain a sramped steel core with cork bonded to each side. If the cork comes off, the sharp steel edge will be exposed.

#### CAUTION:

Care should be taken when hardling this gasket to avoid the possibility of personal injury.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.