HARD HORN BLOW EFFORT 1982 STEERING WHEEL. Buick Electra Estate Wagon 1982

For 1990-2009 cars

# HARD HORN BLOW EFFORT 1982 STEERING WHEEL

#### MODELS AFFECTED: All

Reports have been received that blowing some horns require excessive effort at certain areas of the horn pad.

A repair procedure has been developed to reduce the effort required.

1. Remove horn pad assembly from vehicle.

2. Place pad on work bench with underside up so that area to be modified is supported.

3. Wearing safety glasses, place 4 oz. ballpeen hammer at center of section requiring improvement, and with second hammer strike first hammer hard enough to produce small dent. (See Illustration).

4. Using a self-powered test light, try the areas reworked. If additional improvement is needed, you may repeat this procedure adjacent to previous location.

WARRANTY INFORMATION

LABOR OPERATION NUMBER T5049

LABOR TIME 0.3 HRS.

TROUBLE CODE 92

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.