BROKEN R-AXLE LOCK SCREW REMOVAL TOOL - 'C' LOCK. Buick Electra Estate Wagon 1980

For 1990-2009 cars

# BROKEN R-AXLE LOCK SCREW REMOVAL TOOL - 'C' LOCK

REAR AXLE DIFFERENTIAL PINION SHAFT REMOVER KENT-MOORE TOOL J-35640

#### MODELS AFFECTED: ALL REAR WHEEL DRIVE VEHICLES WITH "C" LOCK --------------- DIFFERENTIAL ASSEMBLIES

Attached is a combination brochure and order form for a new tool released by Kent-Moore to remove a differential pinion shaft when the lock screw is broken. This reasonably priced tool will save technician time and will efficiently remove the pinion shaft without damage to the differential case assembly when the lock screw is broken. This means less vehicle down time and reduced repair expense which translates into increased customer satisfaction.

Kent-Moore will pay freight charges on all J-35640 orders received prior to December 31, 1985.

Please review and route this available tool information to your Service Manager and technicians.

"We believe this source and their products to be reliable. There may be additional manufacturers of such products. Buick does not endorse, indicate any preference for, or assure any, responsibility for the products or equipment from this firm or for any such items which may be available from other sources."

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.