TORQUE SCREW SPECIFICATION NYLON ROCKER ARM COVER. Buick Electra/Park Avenue 1981

For 1990-2009 cars

# TORQUE SCREW SPECIFICATION NYLON ROCKER ARM COVER

GR.6A NYLON ROCKER ARM COVER MOUNTING SCREW/STUD TORQUE SPECIFICATION WHEN SERVICING ALL 1980-81 CADILLAC ENGINES EQUIPPED WITH NYLON ROCKER ARM COVERS, THE NINE ROCKER ARM COVER MOUNTING SCREWS/STUDS SHOULD BE INSTALLED AND TIGHTENED TO 8.0 N.M (71 IN. LBS.). THIS SUPERSEDES THE TORQUE SPECIFICATION PRINTED IN PREVIOUS SERVICE PUBLICATIONS AS WELL AS THE 1981 SERVICE INFORMATION MANUAL.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.