REAR STRUT REMOVAL REVISED PROCEDURE. Buick Electra/Park Avenue 1985

For 1990-2009 cars

# REAR STRUT REMOVAL REVISED PROCEDURE

#### Models Affected: 1985 Electra

The procedure to remove a rear strut from a 1985 Electra has been revised. When removing a rear strut, support the control arm with a jack stand prior to removing any strut fasteners.

Please update page 3D1-5 of your 1985 Chassis Service Manual with this information.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.