NOISE AT INSTRUMENT PANEL REPLACE RETAINING SCREWS. Buick Electra/Park Avenue 1985

For 1990-2009 cars

# NOISE AT INSTRUMENT PANEL REPLACE RETAINING SCREWS

INSTRUMENT PANEL - NOISE AT FRONT OF INSTRUMENT PANEL PAD ASSEMBLY

#### VEHICLES AFFECTED: 1985-87 'C' MODELS; 1986-87 'H' MODELS -----------------

In the event of a recurrence of one or more of the five (5) front attaching screws backing out at the front of the instrument panel pad assembly, correct as follows:

1. Remove instrument panel pad assembly.

2. Replace all five (5) existing J-nuts (See Figure 1, Item A) with new style prevailing torque fastener nuts, Part Number 25530441 available through GM Parts Department. NOTE: THIS NEW PART MAY ALSO BE USED ON OTHER AREAS OF THE INSTRUMENT PANEL CARRIER.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.