POWER STEERING PUMP NOISE SYSTEM PROCEDURE. Buick Electra/Park Avenue 1987

For 1990-2009 cars

# POWER STEERING PUMP NOISE SYSTEM PROCEDURE

#### MODELS AFFECTED: 1986 AND 1987 FRONT WHEEL DRIVE ELECTRAS AND LESABRES

#### NOTICE: This bulletin supersedes Service Bulletin 87-3-2 dated November, 1986, to indicate for proper fill that system should be checked with fluid "hot". Please discard Bulletin 87-3-2.

When servicing the power steering system, pump noise can occur if the system is not properly bled. This is due to air becoming trapped in the system causing pump cavitation. To properly bleed the power steering system, it is important that prior to starting engine, the steering wheel be rotated from stop to stop until no air bubbles appear in the reservoir fluid. In some cases, it may take up to 20 cycles to completely remove the air; therefore, it is recommended that the front wheels be raised off the floor when turning steering wheel.

Power steering fluid should be checked "hot" and filled to the "hot" mark to obtain proper fill.

Except as noted above, the remainder of the bleed procedure on Page 3B3-2, in the 1987 Buick Chassis Service Manual, should be followed.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.