FRONT END NOISE ('POP') ACCELERATION AND/OR BRAKING. Buick Electra/Park Avenue 1985

For 1990-2009 cars

# FRONT END NOISE ('POP') ACCELERATION AND/OR BRAKING

#### Models Affected: 1985 Electra with 3.0L (LK9) and 3.8L MFI (LN3) Engines

#### Notice: This bulletin supersedes 85-10-8 dated October 1984. Note in Step 3 changed. Please discard original bulletin and replace it with this one.

A "squeak, crunch or popping" noise may be experienced on some early Electras acceleration and braking. The condition is usually a single pop.

Follow the recommendations shown in 1983 Dealer Service Bulletin #83-218 in the Body Section along with the following procedures:

1. Remove cradle mounts.

#### Note: Do not disasseable more than two mounts at a time in order to maintain cradle and front end alignment.

2. Squeeze locating guide on the lower cushions slightly, per illustration, in a vise to cause a slight interference fit in the cradle. Rework all six mounts in this manner.

3. Reinstall mounts in the same locations frcm which they were removed.

#### Note: Soap or a soap and water solution may be required to aid installation of top cushion onto lower cushion.

4. Torque cradle mounts to 103 N.m.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.