SPARK PLUG CHANGE ELIMINATES HARD STARTING. Buick Electra/Park Avenue 1984

For 1990-2009 cars

# SPARK PLUG CHANGE ELIMINATES HARD STARTING

#### VEHICLES AFFECTED: 1984 Vehicles Equipped with 5.0L (VIN Code Y or 9)

A - Closed Loop Emission System

Oldsmobile 5.0L V-8 engines built after 10-01-83 and prior to 04-01-84 will be equipped with R46SZ spark plugs with a gap of .060 inches. This change was made to recude cold weather spark plug fouling. The emission label will indicate the correct spark plug as R46SX gapped at .080 inches. Whenever spark plug replacement becomes necessary, the R46SX should be used.

B - Open Loop Emission System

NM6 recalibrated engine will use R47SX gapped at .060 inches for all seasons.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.