FRONT SUSPENSION CASTER ADJUSTMENT PROCEDURE. Buick Electra/Park Avenue 1985

For 1990-2009 cars

# FRONT SUSPENSION CASTER ADJUSTMENT PROCEDURE

MDDELS AFFECTED: 1985 ELECTRAS

To adjust caster on 1985 Electras, it is necessary to file the strut tower in the area shown on page 3A-3 of the "1985 Electra Chassis Service Manual."

For appearance reasons, and corrosion protection, it is important that the area filed be painted with a rust preventative paint, such as Dupont 215S primer or equivalent.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.