3-2 DOWNSHIFT BUMP 440T4 TRANSAXLE,NEW P/N. Buick Electra/Park Avenue 1985

For 1990-2009 cars

# 3-2 DOWNSHIFT BUMP 440T4 TRANSAXLE,NEW P/N

#### MODELS AFFECTED: 1985 CENTURYS AND ELECTRAS WITH 3.8L V-6 ENGINE AND 440-T4 TRANSAXLE

Some 1985 THM 440-T4 "BA" and "BC" model transaxles (refer to Figure 1), may exhibit a 3-2 downshift bump. The condition mayy be most prevalent during a part-throttle downshift with the air conditioner operating.

When servicing any 1985 THM 440-T4 "BA" and "BC" model for a 3-2 downshift bump, order and install service package part number 8646953.

Service package part number 8646953 contains one each of the following:

3-2 Control Valve Spring Instruction Sheet

Refer to Figure 2 of this bulleting and the appropriate chassis service manual for proper installation procedures. NOTICE: This correction does not apply to 19851/2 440-T4 models or to vehicles equipped with 3.0L engines. Refer to chassis service manual 440-T4 diagnosis for shift conditions on other than "BA" or "BC" models.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.