SERVICE MANUAL UPDATE REVISED FLYWHEEL TORQUE SPECS. Buick Electra/Park Avenue 1990

For 1990-2009 cars

# SERVICE MANUAL UPDATE REVISED FLYWHEEL TORQUE SPECS

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 6A - REVISED FLYWHEEL BOLT TORQUE SPECIFICATION

#### MODELS AFFECTED: 1990 REGAL MODELS WITH 3800 (VIN L) ENGINE 1991 SKYLARK AND CENTURY MODELS WITH 3300 (VIN N) ENGINE 1991 PARK AVENUE/ULTRA AND RIVIERA/REATTA MODELS WITH 3800 (VIN L) ENGINE 1991 LESABRE MODELS WITH 3800 (VIN C) ENGINE

The revised flywheel bolt torque specification for the engines listed above is as follows:

Flywheel Bolt to Crankshaft - 15 N.m + 50- (11 ft. lbs. + 50-) Tool Required: J36660 Torque Angle Meter

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.