SERVICE GUILD: SMU SEC. 8A SAFETY BELT RETRACTOR-TEST C. Buick Electra/Park Avenue 1990

For 1990-2009 cars

# SERVICE GUILD: SMU SEC. 8A SAFETY BELT RETRACTOR-TEST C

#### VEHICLES AFFECTED: 1990 C-H CARS

The following statement should be added to C: Safety Belt Retractor Release Solenoid Timer Test:

- Gear Selector Lever: Neutral

This statement should be added to the appropriate Service Manuals as indicated below:

Buick - Page 368 of the Electrical Service Manual. Under second Bullet.

Oldsmobile - Page 8A-146-6 of C-H car manual. Under last bullet.

Pontiac - Page 8A-146-5 of the Bonneville Manual. Under last bullet.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.