STEERING COLUMN NOISE VEHICLES WITH TILT STEERING. Buick Electra/Park Avenue 1984

For 1990-2009 cars

# STEERING COLUMN NOISE VEHICLES WITH TILT STEERING

#### MODELS AFFECTED: 1984

Some 1984 Buick vehicles equipped with tilt steering columns may exhibit a rattling noise in the column. This noise may be from the lock bolt area and can be repaired by lubricating the lock bolt.

1. Remove steering wheel, shaft lock cover, shaft lock, canceling cam, canceling cam spring, signal switch, buzzer switch, lock cylinder and lock housing cover as covered in the 1984 Buick Chassis Service Manual Section 3B4.

2. Liberally coat exposed area of lock bolt with lithium base chassis grease as shown in illustration, then reassemble. Refer to the 1984 Buick Chassis Service Manual Section 3B4 for the reassembly procedure.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.