Ignition and Key Alarm Switch Assembly - Disassemble - Off Vehicle. Buick GL7 (Export) 2000

For 1990-2009 cars

### Disassembly Procedure

1. Remove the upper and lower shrouds. Refer to Steering Column Trim Covers - Disassemble - Off Vehicle .
2. Pop the wire harness assembly (4) out of the wire harness strap (5).
3. Remove the wire harness straps (3) from the wire harness assembly (4).
4. Remove 1 wire harness strap (2) from the upper tilt head assembly (1).
5. Slide the turn signal switch assembly connectors (2) out from the bulk head connector (1).
6. Pull the PASS-Key III off of the lock module assembly (2).
7. Remove the key alarm connector (1) from the lock module assembly (2).
8. Remove the 2 tapping screws from the ignition key alarm switch assembly (3).