Rear Seat Replacement. Buick GL7 (Export) 2000

For 1990-2009 cars

### Removal Procedure

1. Fold the rear seat back flat, except the captain's chair.
2. Slide the rear seat to the most rearward position.
3. Pull the strap on the back side of the rear seat riser in order to release the riser from the floor.
4. Tilt the rear seat fully upwards.
5. Tilt the rear seat rearward and then squeeze the bars together at the front of the seat bottom in order to release the front latch mechanism.
6. Lift the rear seat from the latch.
7. Remove the rear sear from the vehicle.

### Installation Procedure

1. Install the rear seat to the vehicle.
2. Hook the front seat riser latches into the floor.

Ensure that the latch is hooked on both pins.

3. Tilt the rear seat assembly down and latch the rear seat riser latches into the floor.
4. Except the captain's chair, tilt the rear seat back upright.
5. Return the rear seat to its original position.