Vanity Mirror Lamp Replacement. Buick GL7 (Export) 2000

For 1990-2009 cars

### Removal Procedure

1. Use a small, flat-bladed tool in order to remove the lens carefully from the bottom of the lens.
2. Use a small, flat-bladed tool in order to remove the bulb from the socket.

### Installation Procedure

Important: DO NOT touch the glass portion of the bulb. Use a paper towel or a clean shop rag to position the bulb in the socket.

1. Press the bulb into the socket in order to install the bulb.
2. Snap the lens into place.