DTC P0172 Fuel Trim System Rich. Buick GL7 (Export) 2000

For 1990-2009 cars

### Circuit Description

To provide the best possible combination of driveability, fuel economy, and emission control, a Closed Loop air/fuel metering system is used. While in Closed Loop, the powertrain control module (PCM) monitors the heated oxygen sensor (HO2S) 1 signal and adjusts the fuel delivery based upon the HO2S signal voltages. A change made to fuel delivery will be indicated by the long and short term fuel trim values which can be monitored with a scan tool. The ideal fuel trim values are around 0 percent. If the HO2S signals are indicating a lean condition the PCM will add fuel, resulting in fuel trim values of more than 0 percent. If a rich condition is detected, the fuel trim values will be below 0 percent, indicating that the PCM is reducing the amount of fuel delivered. If an excessively rich condition is detected, the PCM will set DTC P0172. The maximum authority of the PCM to control the long term fuel trim allows a range between -25 percent and +20 percent. The maximum authority of the PCM to control the short term fuel trim allows a range between -27 percent and +27 percent. The PCM monitors the fuel trim under various operating conditions, called fuel trim cells, before determining the status of the fuel trim diagnostic. The fuel trim cells are as follows:

Cell | Purge ON | Purge OFF
--- | --- | ---
Idle (Cell 0) | X | --
Decel (Cell 1) | X | --
Normal (Cell 2) | -- | --
Accel (Cell 3) | X | --
High Flow (Cell 4) | -- | --
Long Term FT average less than -25%
Short Term FT less than -3%

The vehicle may have to be operated in all of the above conditions marked by an X, before the PCM determines fuel trim status. The amount of fuel trim deviation from 0 percent in each cell, and the amount that each cell is used, directly affects whether or not the vehicle must be operated in all of the cells described above to complete the diagnostic.

### Conditions for Running the DTC

• | No MAF, ECT, TP, MAP, CMP, CKP, IAT, EVAP, EGR, HO2S, misfire, injector circuit, idle speed, VSS, or IC circuit DTCs are set.

• | The ECT is between 60°C and 110°C (140°F - 230°F).

• | The IAT is between -18°C and +70°C (0°F - 158°F).

• | The MAP is between 15 kPa and 80 kPa.

• | The throttle angle is steady and less than 90 percent.

• | The vehicle speed is less than 132 km/h (82 mph).

• | The engine speed is between 600 and 4000 RPM.

• | The barometric pressure (BARO) is more than 70 kPa.

• | The air flow is between 3 gm/s and 150 gm/s.

### Conditions for Setting the DTC

• | The Long Term Fuel Trim is at or near the maximum authority of -25 percent.

• | The Short Term Fuel Trim is at or near the maximum authority of -3 percent.

• | All the conditions in the Fuel Trim Cells have been met .

### Action Taken When the DTC Sets

• | The PCM will illuminate the malfunction indicator lamp (MIL) during the second consecutive trip in which the diagnostic test has been run and failed.

• | The PCM will store conditions which were present when the DTC set as Freeze Frame/Failure Records data.

### Conditions for Clearing the MIL/DTC

• | The PCM will turn OFF the malfunction indicator lamp (MIL) during the third consecutive trip in which the diagnostic has run and passed.

• | The history DTC will clear after 40 consecutive warm-up cycles have occurred without a malfunction.

• | The DTC can be cleared by using a scan tool.

### Diagnostic Aids

Inspect or test for the following conditions:

• | The fuel pressure is too high. The system will go rich if the pressure is too high. The PCM can compensate for some increase. However, if the fuel pressure is too high, a DTC P0172 may be set. Refer to Fuel System Pressure Test .

• | Any faulty fuel injectors. Refer to Fuel Injector Balance Test .

• | Inspect the EVAP canister for fuel saturation. If the EVAP canister is full of fuel, inspect the canister control and hoses.

• | Disconnect the MAF sensor and see if the rich condition is corrected. If so, replace the MAF sensor. Refer to Mass Airflow Sensor Replacement .

• | Inspect for a leaking fuel pressure regulator diaphragm by checking the vacuum line to the fuel pressure regulator for the presence of fuel.

• | An intermittent TP sensor output will cause the system to go rich due to a false indication of the engine accelerating.

Many situations may lead to an intermittent condition. Perform each inspection or test as directed.

Important: : Remove any debris from the connector surfaces before servicing a component. Inspect the connector gaskets when diagnosing or replacing a component. Ensure that the gaskets are installed correctly. The gaskets prevent contaminate intrusion.

• | Loose terminal connection

- | Use a corresponding mating terminal to test for proper tension. Refer to Testing for Intermittent Conditions and Poor Connections , and to Connector Repairs in Wiring Systems for diagnosis and repair.

- | Inspect the harness connectors for backed out terminals, improper mating, broken locks, improperly formed or damaged terminals, and faulty terminal to wire connection. Refer to Testing for Intermittent Conditions and Poor Connections , and to Connector Repairs in Wiring Systems for diagnosis and repair.

• | Damaged harness--Inspect the wiring harness for damage. If the harness inspection does not reveal a problem, observe the display on the scan tool while moving connectors and wiring harnesses related to the sensor. A change in the scan tool display may indicate the location of the fault. Refer to Wiring Repairs in Wiring Systems for diagnosis and repair.

• | Inspect the powertrain control module (PCM) and the engine grounds for clean and secure connections. Refer to Wiring Repairs in Wiring Systems for diagnosis and repair.

If the condition is determined to be intermittent, reviewing the Snapshot or Freeze Frame/Failure Records may be useful in determining when the DTC or condition was identified.

### Test Description

The numbers below refer to the step numbers on the diagnostic table.

1. Any DTCs other than P0172 may indicate a condition present which may cause a rich condition. If this is the case, repairing the condition which caused the other DTC will most likely correct the DTC P0172.

2. If the DTC P0172 test passes while the Failure Records conditions are being duplicated, the rich condition is intermittent. Refer to Diagnostic Aids or Symptoms for additional information on diagnosing intermittent problems.

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Powertrain On-Board Diagnostic (OBD) System Check? | -- | Go to Step 2 | Go to Powertrain On Board Diagnostic (OBD) System Check
2 | Are any DTCs set other than P0172? | -- | Go to the applicable DTC table | Go to Step 3

3

1. Start and run the vehicle in closed loop.
2. Observe the Long Term FT and the Short Term FT display on the scan tool data list.

Are the displayed values at or near the specified values?

-25% (L.T.)

-3% (S.T.)

Go to Step 5

Go to Step 4

4

1. Review and record the scan tool Failure Records data.
2. Clear the DTC P0172 and operate the vehicle within the Failure Records conditions.
3. Monitor the scan tool Specific DTC info for DTC P0172 while operating the vehicle within the Failure Records conditions.
4. Continue operating the vehicle until the DTC P0172 test runs and note the test result.

Does the scan tool indicate DTC P0172 failed this ignition?

--

Go to Step 5

Go to Diagnostic Aids

5 | Visually and physically inspect the air filter element and replace the filter if necessary. Refer to Air Filter Element Replacement . Did the air filter require replacement? | -- | Go to Step 18 | Go to Step 6
6 | Visually and physically inspect for a collapsed or restricted intake air duct and repair if necessary. Did your inspection reveal a condition requiring repair? | -- | Go to Step 18 | Go to Step 7
7 | Inspect the throttle body inlet screen for damage or for the presence of foreign objects which may partially block airflow through the screen and correct any problem found. Did your inspection of the throttle body reveal a condition requiring repair or replacement? | -- | Go to Step 18 | Go to Step 8
8 | Start the engine and note the idle quality. Is the engine idle low or unsteady ? | -- | Go to Step 9 | Go to Step 12
9 | With the engine idling, observe the IAC count display on the scan tool. Is the IAC value less than the specified value? | 100 | Go to Step 11 | Go to Step 10

10

1. Turn OFF the ignition.
2. Physically inspect the throttle body bore, the throttle plate, and the IAC passages for coking and foreign objects.
3. If a problem is found, repair as necessary.

Did your inspection reveal a condition requiring repair?

--

Go to Step 18

Go to Step 11

11 | Perform the Idle Air Control System Diagnosis. Refer to Idle Air Control (IAC) System Diagnosis . Did you find and correct the condition? | -- | Go to Step 18 | Go to Step 12

12

1. Disconnect the vacuum hose from the fuel pressure regulator and inspect the hose for the presence of fuel.
2. If fuel is present in the vacuum hose, replace the fuel pressure regulator.

Did you find and correct the condition?

--

Go to Step 18

Go to Step 13

13

1. Turn ON the ignition , leaving the engine OFF.
2. Monitor the TP Angle display on the scan tool while slowly depressing the accelerator pedal.

Does the TP Angle display increase steadily and evenly from the minimum value at closed throttle to the maximum value at wide open throttle?

0-100%

Go to Step 14

Go to Step 16

14 | Perform the Fuel System Pressure Test. Refer to Fuel System Pressure Test . Did you find and correct the condition? | -- | Go to Step 18 | Go to Step 15
15 | Perform the Injector Balance Test. Refer to Fuel Injector Balance Test . Did you find and correct the condition? | -- | Go to Step 18 | Go to Step 16

16

1. Remove and visually/physically inspect the HO2S 1 for silicon contamination. Contamination is indicated by a powdery white deposit on the portion of the HO2S that is exposed to the exhaust stream.
2. If contamination is evident, replace the sensor. Refer to Heated Oxygen Sensor Replacement .

Did the sensor require replacement?

--

Go to Step 18

Go to Diagnostic Aids

17 | Replace the TP sensor. Refer to Throttle Position Sensor Replacement . Did you complete the replacement? | -- | Go to Step 18 | --

18

1. Review and record the scan tool Failure Records data.
2. Clear the DTC P0172 and operate the vehicle within the Failure Records conditions.
3. Monitor the scan tool Specific DTC info for DTC P0172 while operating the vehicle within the Failure Records conditions.
4. Continue operating the vehicle until the DTC P0172 test runs and note the test result.

Does the scan tool indicate DTC P0172 failed this ignition?

--

Go to Step 2

System OK