Radio Setup. Buick GL7 (Export) 2000

For 1990-2009 cars

### Radio Setup

For the DE 100 series radio, complete the following procedure, with the key in the ON position use a scan tool, in order to properly set up communication:

1. At the Main Menu screen, select F0: Diagnostics.
2. At the Vehicle Identification screen, select the following options:

2.1. | 2000 (Model Year)

2.2. | LD Trk, MPV, Incomplete

3. At the System Selection Menu screen, select F1: Body.
4. At the Vehicle Identification screen, select U or X (Platform type).
5. At the Body screen, select F3: Radio.
6. At the Radio screen, select F1: Special Functions.
7. At the Special Functions screen, select F4: Radio Setup.
8. Select the appropriate radio. Uplevel Radio is anything other than the Base AM/FM Radio.

Important: The F4: Radio Setup option does not contain a submenu. Radio Setup will configure the following systems:

• | Steering wheel controls

• | Learn VIN

• | DTCs

• | Class 2 radio messages

### Radio Tuner Calibration

In order to calibrate the radio, begin at the Special Functions screen. Repeat step 1 through step 7 of the Radio Setup, if needed.

At the Special Functions screen, select F2: Country Code.

Important: The F2: Country Code option does not contain a submenu. Country Code sets the point of sale, or origin, in the radio in order to calibrate the tuner for the country that the vehicle will be used in.

### Radio Chime Volume Selection

In order to set the chime volume, begin at the Special Functions screen. Repeat step 1 through step 7 of the Radio Setup, if needed.

1. At the Special Functions screen, select F1: Set Options.
2. At the Set Options screen, select F0: Chime Settings.
3. At the Chime Settings screen, select the following option:

• | F1: Loud Chime Volume

• | Select the appropriate voltage/volume level.

Important: The F1: Loud Chime Volume option does not contain a submenu. This selection is used for setting the volume when the radio is replaced.

### Radio Chime Level Selection

In order to set the Chime Level, begin at the Special Functions screen. Repeat step 1 through step 7 of the Radio Setup, if needed.

1. At the Special Functions screen, select F1: Set Options.
2. At the Set Options screen, select F0: Chime Settings.
3. At the Chime Settings screen, select F0: Chime Level.

Important: The F0: Chime Level option does not contain a submenu. The Chime Level setting has an option of setting a normal chime or a loud chime when the radio is replaced.