Charge Indicator Inoperative. Buick GL7 (Export) 2000

For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you perform the Diagnostic System Check - Starting and Charging? | Go to step 2 | Go to Diagnostic System Check - Engine Electrical

2

1. Turn OFF the ignition.
2. Turn ON the ignition, with the engine OFF.

Does the battery charge indicator illuminate during the bulb check?

Go to Testing for Intermittent Conditions and Poor Connections in Wiring Systems

Go to step 3

3 | Replace the instrument panel cluster. Refer to Instrument Cluster Replacement in Instrument Panel, Gauges and Console. Did you complete the replacement? | Go to step 4 | --
4 | Operate the system for which the symptom occurred. Did you correct the condition? | System OK | Go to step 2