Keyless Entry System Operation. Buick GL7 (Export) 2000

For 1990-2009 cars

### Unlock Driver's Door Only

(BCM MODE 2 ONLY) Momentarily press the UNLOCK button on the keyless entry transmitter in order to perform the following functions:

• | Unlock the driver's door only.

• | Illuminate the interior lamps for approximately 40 seconds or until the ignition is turned ON.

### Unlock All Doors

(BCM MODE 2 ONLY) Momentarily press the UNLOCK button a second time within 5 seconds of the first press in order to perform the following functions:

• | Unlock the remaining doors.

• | Illuminate the interior lamps for approximately 40 seconds or until the ignition is turned ON.

(BCM MODE 1 ONLY) Momentarily press the UNLOCK button in order to perform the following functions:

• | Unlock all of the doors, including the driver's door.

• | Illuminate the interior lamps for approximately 40 seconds or until the ignition is turned ON.

### Lock All Doors

Press the LOCK button in order to perform the following functions:

• | Lock all of the doors.

• | Immediately turn off the interior lamps.

For further information, refer to Keyless Entry System Circuit Description .