Front Bumper Fascia Replacement. Buick GL7 (Export) 2000

For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 38778 Door Trim Pad and Garnish Clip Remover

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove both of the front tire and wheels.
3. Remove the right and left front fender liner. Refer to Fender Liner Replacement in Body Front End.
4. Remove the front park/turn signal/side marker lamp. Refer to Parking and Turn Signal Lamp Replacement in Lighting Systems.
5. Remove the push-in retainers from the upper and lower front bumper fascia.
6. Remove the front bumper fascia from the vehicle.

### Installation Procedure

1. Align the front bumper to the front impact bar and to the body.
2. Install the push-in retainers to the upper and lower front bumper fascia.
3. Install the front park/turn signal/sidemarker lamp. Refer to Parking and Turn Signal Lamp Replacement in Lighting Systems.
4. Install the right and left front fender liner. Refer to Fender Liner Replacement in Body Front End.
5. Install both of the front tire and wheels.
6. Lower the vehicle.