Front Side Door Auxiliary Sealing Strip Replacement. Buick GL7 (Export) 2000

For 1990-2009 cars

### Removal Procedure

1. Use a heat gun in order to heat the front door auxiliary weather-strip.

1.1. | Hold the heat gun approximately 152 mm (6 in) from the surface.

1.2. | Apply the heat using a circular motion for approximately 30 seconds.

2. Use a flat-bladed tool in order to peel the front door auxiliary weather-strip from the panel surface.
3. Do not damage the paint during removal of the auxiliary weather-strip.
4. Use oil-free naphtha in order to clean the body panel.

### Installation Procedure

1. Warm the body panel with a heat lamp or heat gun to a minimum temperature of 21°C (70°F).
2. Peel the backing from the front end of the front door auxiliary weather-strip.
3. Do not touch the adhesive backing.
4. Press the front door auxiliary weather-strip to the body as you continue to remove the backing.
5. Hand roll the front door auxiliary weather-strip to the body in order to ensure proper adhesion.