Body Side Rear Upper Garnish Molding Replacement. Buick GL7 (Export) 2000

For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 38778 Door Trim Pad and Garnish Clip Remover

1. Remove the seat belt shoulder belt guide loop. Refer to Front Seat Shoulder Belt Guide Adjuster Replacement in Seat Belts.
2. Remove the body pillar upper trim panel retainers using the J 38778 .
3. Remove the body pillar upper trim panel by pulling the panel from the locator tabs.

### Installation Procedure

1. Align the locator tabs on the body pillar upper trim panel with the rear quarter trim panel.
2. Align the body pillar upper trim panel retainers with the holes and push to secure the panel to the vehicle.
3. Align the slider door seal to the body pillar upper trim panel if applicable.
4. Install the seat belt shoulder belt guide loop. Refer to Front Seat Shoulder Belt Guide Adjuster Replacement in Seat Belts.