Rear Window Defogger Relay Replacement. Buick GL7 (Export) 2000

For 1990-2009 cars

### Removal Procedure

1. Remove the right side instrument panel insulator panel. Refer to Instrument Panel Insulator Panel Replacement - Right Side in Instrument Panel, Gauges and Console.
2. Remove the rear window defogger timer/relay (1,2) from the relay block.

### Installation Procedure

1. Install the rear window defogger timer/relay (1,2) into the relay block.
2. Install the right side instrument panel insulator panel. Refer to Instrument Panel Insulator Panel Replacement - Right Side in Instrument Panel, Gauges and Console.