Fastener Tightening Specifications. Buick GL7 (Export) 2000

For 1990-2009 cars

Application | Specifications
--- | ---
Metric | English
Accelerator Control Cable Bracket Bolt/Nut | 10 N·m | 89 lb in
Camshaft Position Sensor Bolt | 10 N·m | 89 lb in
Camshaft Sprocket Bolt | 140 N·m | 103 lb ft
Camshaft Thrust Plate Screw | 10 N·m | 89 lb in
Connecting Rod Bearing Cap Bolt

- First Pass

25 N·m

18 lb ft

- Final Pass

100 degrees

Coolant Drain Plug | 19 N·m | 14 lb ft
Coolant Temperature Sensor | 23 N·m | 17 lb ft
Crankshaft Balancer Bolt | 103 N·m | 76 lb ft
Crankshaft Main Bearing Cap Bolt/Stud

- First Pass

50 N·m

37 lb ft

- Final Pass

77 degrees

Crankshaft Oil Deflector Nut | 25 N·m | 18 lb ft
Crankshaft Position Sensor Bolt -- Front Cover | 10 N·m | 89 lb in
Crankshaft Position Sensor Stud -- Side of Engine Block | 11 N·m | 98 lb in
Crankshaft Position Sensor Wiring Bracket Bolt | 50 N·m | 37 lb ft
Cylinder Head Bolt

- First Pass

50 N·m

37 lb ft

- Final Pass

90 degrees

Drive Belt Shield Bolt | 10 N·m | 89 lb in
Drive Belt Tensioner Bolt | 50 N·m | 37 lb ft
EGR Valve Bolts | 30 N·m | 18 lb ft
EGR Valve Pipe | 25 N·m | 18 lb ft
Engine Flywheel Bolt | 71 N·m | 52 lb ft
Engine Front Cover Bolt -- Large | 55 N·m | 41 lb ft
Engine Front Cover Bolt -- Medium | 47 N·m | 35 lb ft
Engine Front Cover Bolt -- Small | 21 N·m | 15 lb ft
Engine Mount Bracket Bolt | 58 N·m | 43 lb ft
Engine Mount Lower Nut | 43 N·m | 32 lb ft
Engine Mount Strut and Lift Bracket Bolt -- Engine Left Rear | 70 N·m | 52 lb ft
Engine Mount Strut Bolt/Nut | 48 N·m | 35 lb ft
Engine Mount Strut Bracket Bolt -- Upper Radiator Support | 28 N·m | 21 lb ft
Engine Mount Strut Bracket Bolt -- Vehicle Right Side | 50 N·m | 37 lb ft
Engine Mount Upper Nut | 47 N·m | 35 lb ft
Engine Oil Pressure Indicator Switch | 13 N·m | 115 lb in
Engine Wiring Harness Bracket Bolt | 13 N·m | 115 lb in
Exhaust Crossover Pipe Heat Shield Bolt | 10 N·m | 89 lb in
Exhaust Crossover Pipe Nut/Stud | 25 N·m | 18 lb ft
Exhaust Manifold Heat Shield Bolt | 10 N·m | 89 lb in
Exhaust Manifold Nut | 16 N·m | 12 lb ft
Exhaust Manifold Stud | 18 N·m | 13 lb ft
Fuel Feed Pipe to Fuel Injector Rail Nut | 17 N·m | 13 lb ft
Fuel Injector Rail Bolt | 10 N·m | 89 lb in
Fuel Pipe Bracket Bolt/Stud | 50 N·m | 37 lb ft
Fuel Pipe Clip Bolt | 8 N·m | 71 lb in
Fuel Return Pipe to Fuel Injector Rail Nut | 17 N·m | 13 lb ft
Generator Bracket and Front Engine Lift Hook Bolt | 50 N·m | 37 lb ft
Heater Inlet Pipe Nut | 25 N·m | 18 lb ft
Ignition Coil Bracket Bolt/Nut/Stud | 25 N·m | 18 lb ft
Intake Manifold Coolant Pipe Bolt | 10 N·m | 89 lb in
Knock Sensor | 19 N·m | 14 lb ft
Lower Intake Manifold Bolt | 13 N·m | 115 lb in
MAP Sensor Bracket Bolt | 25 N·m | 18 lb ft
MAP Sensor Bolt | 5 N·m | 44 lb in
Oil Cooler Connector | 50 N·m | 37 lb ft
Oil Cooler Hose Fitting | 19 N·m | 14 lb ft
Oil Cooler Pipe Bracket Bolt | 10 N·m | 89 lb in
Oil Filter | 13 N·m | 115 lb in
Oil Filter Bypass Hole Plug | 19 N·m | 14 lb ft
Oil Filter Fitting | 39 N·m | 29 lb ft
Oil Gallery Plug -- 1/4 inch | 19 N·m | 14 lb ft
Oil Gallery Plug -- 3/8 inch | 33 N·m | 24 lb ft
Oil Level Indicator Tube Stud | 25 N·m | 18 lb ft
Oil Level Sensor Bolt | 10 N·m | 89 lb in
Oil Pan Bolt | 25 N·m | 18 lb ft
Oil Pan Drain Plug | 25 N·m | 18 lb ft
Oil Pan Side Bolt | 50 N·m | 37 lb ft
Oil Pump Cover Bolt | 10 N·m | 89 lb in
Oil Pump Drive Clamp Bolt | 36 N·m | 27 lb ft
Oil Pump Mounting Bolt | 41 N·m | 30 lb ft
Spark Plug

- Spark Plug - Initial Installation

20 N·m

15 lb ft

- Spark Plug - Reinstallation

15 N·m

11 lb ft

Thermostat Bypass Pipe to Cylinder Head Nut | 25 N·m | 18 lb ft
Thermostat Bypass Pipe to Engine Front Cover Bolt | 12 N·m | 106 lb in
Thermostat Bypass Pipe to Throttle Body Nut | 25 N·m | 18 lb ft
Throttle Body Bolt/Stud | 25 N·m | 18 lb ft
Timing Chain Dampener Bolt | 21 N·m | 15 lb ft
Upper Intake Manifold Bolt/Stud | 25 N·m | 18 lb ft
Valve Lifter Guide Bolt | 10 N·m | 89 lb in
Valve Rocker Arm Bolt

- First Pass

19 N·m

14 lb ft

- Final Pass

30 degrees

Valve Rocker Arm Cover Bolt | 10 N·m | 89 lb in
Water Outlet Bolt | 25 N·m | 18 lb ft
Water Pump Bolt | 10 N·m | 89 lb in
Water Pump Pulley Bolt | 25 N·m | 18 lb ft