Engine Mount Strut Bracket Installation. Buick GL7 (Export) 2000

For 1990-2009 cars

## Engine Mount Strut Bracket Installation Generator Bracket

1. Install the front engine lift bracket.
2. Install the generator bracket.
3. Install the generator bracket bolts

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

Tighten
Tighten the generator bracket bolts in sequence (1,2,3,4) to 50 N·m (37 lb ft).

## Engine Mount Strut Bracket Installation and Rear Engine Lift Bracket

1. Install the engine mount strut and lift bracket.
2. Install the engine mount strut and lift bracket bolts.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

Tighten
Tighten the engine mount strut and lift bracket bolts to 70 N·m (52 lb ft).