Radiator Outlet Hose Replacement. Buick GL7 (Export) 2000

For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 38185 Hose Clamp Pliers

1. Drain the coolant. Refer to Cooling System Draining and Filling .
2. Disconnect the outlet hose from (3) the water pump housing (1) using the J 38185 .
3. Disconnect the outlet hose (3) from the radiator (2) using the J 38185 .
4. Remove the outlet hose.

### Installation Procedure

1. Install the outlet hose in position and align the marks on the hose.
2. Connect the outlet hose (3) to the radiator (2) using the J 38185 .
3. Connect the outlet hose (3) to the water pump housing (1) using the J 38185 .

Important: To properly fill the system you must use of the air bleed vents. Refer to Cooling System Draining and Filling .

4. Refill the coolant. Refer to Cooling System Draining and Filling .