Accelerator Pedal Replacement. Buick GL7 (Export) 2000

For 1990-2009 cars

### Removal Procedure

1. Remove the left instrument panel sound insulator. Refer to Instrument Panel Insulator Panel Replacement - Left Side in Instrument Panel, Gauges, and Console.
2. Disconnect the accelerator cable from accelerator pedal.
3. Remove the bolts and studs holding the accelerator pedal to the bulk head.
4. Remove the accelerator pedal.

### Installation Procedure

1. Position the accelerator pedal to the bulkhead.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Reinstall the accelerator pedal bolt and stud.

Tighten
Tighten the bolts and the studs to 3.0 N·m (27 lb in).

3. Connect the accelerator cable to accelerator pedal.
4. Check for complete throttle opening and closing positions by operating the accelerator pedal. Also inspect the carpet fit under the accelerator pedal.
5. Reinstall the left instrument panel sound insulator. Refer to Instrument Panel Insulator Panel Replacement - Left Side in Instrument Panel, Gauges, and Console.