Manifold Absolute Pressure Sensor Replacement. Buick GL7 (Export) 2000

For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable Battery Negative Cable Disconnection and Connection in Engine Electrical
2. Remove the bolt/screws (6).
3. Disconnect the electrical connector.
4. Disconnect the inlet vacuum hose (7).
5. Remove the MAP sensor (5) from the bracket (2)

### Installation Procedure

1. Install the MAP sensor (5) to the bracket.
2. Connect the electrical connector.
3. Connect the inlet vacuum hose (7).
4. Connect the negative battery cable.