RPO Code List. Buick GL7 (Export) 2000

For 1990-2009 cars

The following table provides the description of the Regular Production Option (RPO) codes that are available on the vehicle. The vehicle's RPO list is printed on the Service Parts Identification Label.

RPO | Description
--- | ---
AK5 | Restraint System Front Seat, Inflatable, Driver and Passenger (Unique SGM China requirement
AL4 | Seat RR BKT
AM7 | Seat Rr Folding (3-Pass Solid Bench ) (3rd Row) Unique SGM China requirement
AP9 | Restraint Cargo (Convenience Net - Cross Cargo Area) (Chev Req. Y91)
AR9 | Seat FRT BKT, Deluxe
AT5 | Seat Rr Center, Folding 2-Pass 40/60 Bench, (2nd Row)
AU0 | Lock Control Remote Entry (RFA) (Int Lights - On/Fade Off)
AX4 | Restraints Conversion Seat, Man. (Shoulder Belt Restraints) Euro
A26 | Windshield, European Glazing
A31 | Window Power-Operated Side; Domestic Inc.: Express Down; GME Inc. Auto Down/Auto Up/Anti-jam
BA8 | Compartment Stowage, FRT Seat, Pass
BG9 | Covering Floor Rubber (Req. Z10/9C6)
BS1 | Insulation Acquostical PKG
B37 | Covering Floor MAT, FRT and RR, AUX
CKD | Vehicle, Knocked Down (Unique SGM China requirement)
CZ2 | Country China
C25 | Wiper, Rear w/Fixed Delay/Wash
C3L | GVW Rating 5357 LBS
C34 | HVAC System Air Conditioner Heater Combination (Frt/Rr w/Rear Controls)
C49 | Defogger Rear Window Electric
C79 | Lamp Interior, Roof Rail, Courtesy & Single Reading (Rows 2/3 - SSD/Row 3 - DDS) (Chev Req. Y91)
DD9 | Mirror, Outside LH/RH Remote Control, Electric, Breakaway, Painted (Black), Unique SGM China requirement
DK6 | Console, Interior Roof (Ext. - Inc. DIC) (Chev Req. Y91)
D55 | Console, Frt, Compt, Flr
EXP | Export
E28 | Assist Grips, B-Pillar-Mounted
FE2 | Suspension System Ride, Handling (Pontiac)
FR9 | Ratio Transaxle Final Drive 3.29 (Req. LA1)
GQ1 | Axle Rear Standard Ratio
IPB | Trim Interior Design
JL9 | Brake System Power, Frt/Rf Disc Antilock, Frt/Rr Wheel
K12 | Filter, Odor/Pollen
K45 | Air Cleaner, Heavy Duty
KG9 | Generator, 140 amp (Unique SGM China requirement)
LW9 | Engine, Gas, 6 Cyl. 3.0L, SFI, V6, HO, (Unleaded) (Unique SGM China requirement)
MD7 | Transmission Auto 4-SPD, HMD, 4T65-E Shanghai, O/D
MXO | Merchandised Trans Auto Provisions, O/D
NB8 | Emission Override California System
NC7 | Emission Override Federal System
NF2 | Emission Override Federal System
NP7 | Steering Column EEC Approved (Energy Absorbing) (GME Req. CV5)
NV6 | Steering Power, Reduced Effort
NY8 | Shield Exhaust
N30 | Steering Wheel Deluxe
PG1 | Wheels 15 x 6, Steel
PH3 | Wheels 15 x 6, Aluminum Cast, 115 mm Bolt Circle
SHC | Plant Code Shanghai, China
TL4 | Grille Painted
T2H | Ornamentation Exterior, Export Unique Req. (Unique SGM China Requirement)
T2J | Ornamentation Interior, Export Unique Requirements
T84 | Headlamps, RH Rule of Road (E Mark Rectangular) (LHD), Export, Halogen (Inc. Motors for leveling for GME)
T89 | Lamp Tail and Stop, Export (w/Integral Fog Lamps)
T90 | Lamps, Signaling and Marker Export
UH8 | Cluster Instrument, Coolant Temperature, Trip Odometer, Tachometer
UL2 | Frequencies, European Radio
UZ5 | Speaker System, 4 Dual Front Door Coaxial, Dual Rear Liftgate Coaxial
U1N | Radio AM/FM Stereo, seek/scan, auto reverse, music, search cass., clock, eqlzr, RDS, ETR
U1P | Radio AM/FM Stereo, seek/scan, CD, clock, eqlzr, RDS, ETR
U18 | Speedometer Instrument, Kilo (Europe)
U29 | Lamp INTR, I/P Courtesy
U76 | Antenna, Windshield Radio
VH7 | Bumper, Custom (GME Req. Y93/Y94)
V2G | Credit Full Fuel Fill
V76 | Hook Tow
V78 | Vehicle Statement
W82 | Equipment MISC EQUIP for China PTR (China Controlled)
W83 | Equipment MISC EQUIP for China
XPK | Tire Frt P215/70R15 BW R/PE ST TL ALS 97S
YB6 | Axle (Base EQUIP)
YD5 | Spring Front Base Equipment
YD6 | Spring Rear Base Equipment
Y1F | Primary Color Exterior, Fleet Yellow (Chev Req. 9C6 - taxi, Opel - optional)
ZP7 | Seating Arrangement 7 passenger, Row 1: Front Buckets-2; Row 2: 60/40 bench seats-2 (RPO: AT5), Row 3: Solid bench - k3 (RPO: AM7) (Unique SGM China requirement)
09U | Primary Color Exterior, Crimson King Metallic (Req. D89 Exc. Chev)
14B | Trim Combination Cloth Light Gray (B) (92)
14C | Trim Combination Cloth Light Gray (C) (Chev Req. Y91)
14I | Interior Trim Light Gray (I) (92)
16U | Primary Color Exterior, Bright White (Req. D89 Exc. Chev)
28U | Primary Color Exterior, Black Sapphire Metallic (Pont/IPC Exp Req. D84)
642 | Trim Combination, Leather, Medium Dark Sable