Fuel Level Sensor Replacement. Buick GL7 (Export) 2000

For 1990-2009 cars

### Removal Procedure

1. Remove the fuel sender assembly. Refer to Fuel Sender Assembly Replacement .
2. Press the fuel level sender retainer tabs together to release the sender.
3. Remove the fuel level sensor (5) from the modular fuel sender.

### Installation Procedure

1. Install the fuel level sensor (5) to the modular fuel sender.
2. Install the fuel sender assembly. Refer to Fuel Sender Assembly Replacement .