Inflatable Restraint Steering Wheel Module Coil Assemble - Off Vehicle. Buick GL7 (Export) 2000

For 1990-2009 cars

### Assembly Procedure

1. Install the wave washer (1).
2. Align the block tooth on the race and upper shaft assembly (1) to the 12 o'clock position.
3. Put the lock cylinder in the LOCK position and remove the key.
4. A new SRS coil assembly will be precentered. Do not remove the centering tab until installation is complete.
5. If reusing the original SRS coil assembly refer to Inflatable Restraint Coil Centering - Off Vehicle (Column Shift and Floor Shift) .
6. Align the SRS coil assembly (2) with the horn tower sticking through the shaft lock shield assembly (1).

Important: The snap ring (1) must seat securely on the groove of the race and upper shaft assembly (2).

7. Install the snap ring (1).
8. Pop the wire harness assembly (4) into the wire harness strap (5).
9. Install the wire harness strap (2) into the steering column tilt head assembly (1).
10. Install the wire harness straps (3) onto the wire harness assembly (4).
11. Install the upper and lower shrouds. Refer to Steering Column Trim Covers - Assemble - Off Vehicle .