Parking and Turn Signal Lamp Replacement. Buick GL7 (Export) 2000

For 1990-2009 cars

### Removal Procedure

1. Open the hood.
2. Remove the wiring nut from the Headlamp bracket to front park/turn signal/sidemarker lamp bracket.
3. Remove the front park/turn signal/sidemarker lamp from the body.
4. Press the tab while turning counterclockwise in order to unscrew the bulb socket from the front park/turn signal/sidemarker lamp.
5. Pull the bulb from the socket.

### Installation Procedure

1. Press the bulb into the socket.
2. Install the socket to the front park/turn signal/sidemarker lamp.
3. Install the front park/turn signal/sidemarker lamp to the body:

3.1. | Locate the tabs into the fender.

3.2. | Install the tab into the Headlamp bracket.

4. Install the wiring nut to Headlamp bracket to the front park/turn signal/sidemarker lamp bracket.
5. Close the hood.