Engine Cooling System Specifications. Buick GL7 (Export) 2000

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Antifreeze | GM Goodwrench DEX-COOL® or HAVOLINE® DEX-COOL®
Antifreeze to Water Ratio | 56% GM Goodwrench DEX-COOL® or HAVOLINE® DEX-COOL® to 44% Water
Coolant Freeze Point Protection | -35°C (-32°F) to -45°C (-48°F)
Cooling System Capacities

- Front HVAC System Only (C60)

9.1 liters

9.5 quarts

- Front and Rear HVAC System (C34)

11.6 liters

12.1 quarts

- Coolant Recovery Reservoir

0.99 liters

1 quart

- Cooling Fan Blade Diameter

360 mm

14.1 in

- Motor Type

Generation II Low Profile Permanent Magnet