Front Side Door Water Deflector Replacement. Buick GL7 (Export) 2000

For 1990-2009 cars

### Removal Procedure

1. Remove the front door trim panel. Refer to Door Trim Panel Replacement .

Important: The water deflector is stuck to the inner door with adhesive tape and is very sticky. Use caution when removing not to rip the water deflector.

2. Carefully peel off the water deflector.

### Installation Procedure

Important: Proper adhesive bonding of the front door water deflector to the inner panel is critical in order to prevent water leaks.

1. Roll the water deflector onto the door panel.
2. Install the front door trim panel. Refer to Door Trim Panel Replacement .