Rear Side Door Water Deflector Replacement. Buick GL7 (Export) 2000

For 1990-2009 cars

### Removal Procedure

1. Remove the sliding door inner trim panel. Refer to Sliding Door Inner Trim Panel Replacement .
2. Carefully peel the water deflector from the door.

### Installation Procedure

Important: Ensure proper adhesive bonding of the sliding door water deflector to the inner panel. Proper adhesive bonding helps to prevent water leaks.

1. Install the water deflector to the door. Use a roller in order to properly set the adhesive to the door panel.
2. Install the sliding door inner trim panel. Refer to Sliding Door Inner Trim Panel Replacement .