Steering Linkage Outer Tie Rod Replacement. Buick GL7 (Export) 2000

For 1990-2009 cars

### Disassembly Procedure

#### Tools Required

J 24319-01 J 24319-01 Universal Steering Linkage Puller

1. Pull the prevailing torque nut (2) from outer tie rod assembly (1).
2. Loosen the jam nut (2) on the inner tie rod assembly (1).
3. Remove the outer tie rod assembly (2) from the steering knuckle (1) using J 24319-01 J 24319-01.
4. Remove the outer tie rod assembly (3) from the inner tie rod assembly (1).

### Assembly Procedure

1. Connect the outer tie rod assembly (3) to the inner tie rod (1).
2. Do not tighten the jam nut (2).
3. Connect the outer tie rod assembly (2) to the steering knuckle (1).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

Important: Be sure the rack and pinion boot is not twisted or puckered during toe adjustment.

4. Connect the prevailing torque nut (2) to the outer tie rod stud (1).

Tighten
Tighten the prevailing torque nut (2) to 25 N·m (18 lb ft). Tighten the prevailing torque nut (2) an additional 180 degrees of rotation.

Tighten
Tighten the jam nut against the outer tie rod to 68 N·m (50 lb ft).