Fastener Tightening Specifications. Buick GL7 (Export) 2000

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
A/C Refrigerant Pressure Sensor | 5 N·m | 44 lb in
Accelerator Cable Bracket Retaining Nuts and Bolts | 10 N·m | 7 lb ft
Camshaft Position Sensor Retaining Bolt | 10 N·m | 7 lb ft
Crankshaft Balancer Bolt | 102.5 N·m | 76 lb ft
Crankshaft Position 7X Sensor Bolt | 11 N·m | 8 lb ft
Crankshaft Position 24X Sensor Bolt | 10 N·m | 7 lb ft
EGR Valve to Throttle Body Adapter Bolts | 30 N·m | 22 lb ft
Engine Coolant Temperature Sensor | 22 N·m | 17 lb ft
Engine Oil Level Switch | 22 N·m | 17 lb ft
Engine Oil Pressure Indicator | 16 N·m | 12 lb ft
EVAP Fuel Filler Pipe Hose Clamp | 2.5 N·m | 22 lb in
EVAP Purge Valve Bracket | 10 N·m | 7 lb ft
Fuel Filler Pipe Hose Clamp | 2.5 N·m | 22 lb in
Fuel Rail Attaching Nuts or Bolts | 10 N·m | 7 lb ft
Fuel Tank Retaining Strap Bolts | 48 N·m | 35 lb ft
Heated Oxygen Sensor | 41 N·m | 30 lb ft
Idle Air Control Valve Attaching Screws | 3 N·m | 27 lb in
Ignition Coil to Ignition Control Module Screws | 4.5 N·m | 40 lb in
Ignition Control Module Bracket to Engine Studs and Nuts | 25 N·m | 18 lb ft
In-pipe Fuel Filter Outlet Nut | 30 N·m | 22 lb ft
Knock Sensor | 19 N·m | 14 lb in
Manifold Absolute Pressure Sensor Retaining Bolt | 5 N·m | 44 lb in
Spark Plugs | 27 N·m | 20 lb ft
Throttle Body Retaining Nuts or Bolts | 25 N·m | 18 lb ft
Throttle Position Sensor Screws | 2 N·m | 18 lb in
Transaxle Range Switch Attaching Bolts | 28 N·m | 20 lb ft
Upper Intake Manifold Studs or Bolts | 25 N·m | 18 lb ft