Steering Column Tilt Head Housing - Disassemble - Off Vehicle. Buick GL7 (Export) 2000

For 1990-2009 cars

### Disassembly Procedure

#### Tools Required

J 23653-SIR Lock Plate Compressor

1. Remove the SRS coil assembly. Refer to Inflatable Restraint Steering Wheel Module Coil Disassemble - Off Vehicle .
2. Remove the bearing retainer using J 23653-SIR and dispose of it.
3. Remove J 23653-SIR from the steering column.
4. Remove the shaft lock shield assembly (1).
5. Remove the turn signal cancel cam assembly (2).
6. Remove the upper bearing spring (3).
7. Remove the upper bearing inner race (4).
8. Remove the inner race (5).