Front Bumper Fascia Support Replacement. Buick GL7 (Export) 2000

For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 38778 Door Trim Pad and Garnish Clip Remover

1. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement .
2. Use J 38778 in order to remove the push-in retainers from the front bumper fascia lower support.
3. Remove the front bumper fascia lower support from the front impact bar.

### Installation Procedure

1. Install the front bumper fascia lower support to the front impact bar.
2. Install the push-in retainers to the front bumper fascia lower support.
3. Install the front bumper fascia. Refer to Front Bumper Fascia Replacement .