DTC B0026 LF/Driver Frontal Deployment Loop (Single Stage or Stage 1) Open. Buick GL7 (Export) 2000

For 1990-2009 cars
Power, Ground, DLC, and SIR Lamp
SIR Handling Caution

### Circuit Description

When you first turn ON the ignition, the inflatable restraint sensing and diagnostic module (SDM) performs tests to diagnose critical malfunctions within itself. Then the SDM performs the following continuous diagnostic tests on the deployment loops:

• | Deployment loop voltage out of range test

• | Deployment loop resistance measurement test

If the voltage out of range test detects a short to voltage condition, the resistance measurement test for that deployment loop will not be performed.

### Conditions for Running the DTC

Deployment loop voltage out of range test:

• | Ignition 1 voltage is within the normal operating voltage range.

• | Driver deployment loop is not shorted to voltage.

• | Driver high terminal A6 is less than 2 volts.

Deployment loop resistance measurement test:

• | Ignition 1 voltage is within the normal operating voltage range.

• | Driver deployment loop is not shorted to voltage.

• | Driver deployment loop is not shorted to ground.

### Conditions for Setting the DTC

Deployment loop voltage out of range test - Driver deployment loop resistance is at least 6 ohms for 300 milliseconds.

Deployment loop resistance measurement test - Driver deployment loop resistance is more than 4.8 ohms for 300 milliseconds.

### Action Taken When the DTC Sets

The SDM commands ON the AIR BAG warning lamp via Class 2 serial data.

### Conditions for Clearing the DTC

• | You can issue a CLEAR CODES command

• | A history DTC will clear once 255 malfunction free ignition cycles have occurred

### Diagnostic Aids

The following can cuase an intermittent condition:

• | The inflatable restraint steering wheel module 2-way connector.

• | The inflatable restraint steering wheel module coil 2-way harness connector.

• | The SDM wiring harness connector.

• | The wire to terminal connections in the driver high circuit.

• | The wire to terminal connections in the driver low circuit.

• | Refer to Testing for Intermittent Conditions and Poor Connections in Wiring Systems.

### Test Description

The number(s) below refer to the step number(s) on the diagnostic table.

1. This step checks the inline connector C215.

2. This step determines if the inflatable restraint steering wheel module coil or the inflatable restraint steering wheel module is defective.

3. This step checks to see if the SDM wiring harness connector is OK.

4. This step checks to see if there is an open or a high resistance in the driver high circuit.

5. This step determines if there is an open or a high resistance in the driver low circuit or if there is a malfunctioning SDM.

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform A Diagnostic System Check - SIR? | -- | Go to Step 2 | Go to Diagnostic System Check - SIR

2

1. Turn OFF the ignition.
2. Disconnect the inflatable restraint steering wheel module coil inline connector C215. Refer to Inflatable Restraint Steering Wheel Module Coil Replacement .
3. Inspect the male and female sides of the inline connector for the following conditions:

• | Corrosion

• | Damaged terminals

• | Poor connections/terminal tension

4. Refer to Testing for Intermittent Conditions and Poor Connections in Wiring Systems.

Does either the male or female side of the inline connector exhibit signs of corrosion, terminal damage, or poor connections?

--

Go to Step 4

Go to Step 3

3

1. If the female side of the inline connector is damaged, the inflatable restraint steering wheel module must be replaced.
2. If the male side of the inline connector is damaged, replace the male side of the inline connector. Refer to Connector Repairs in Wiring Systems.

Did you complete the repair?

--

Go to Step 16

--

4

1. Reconnect the 2-way inline connector.
2. Verify that the connector position assurance (CPA) is properly installed.
3. Turn ON the ignition, with the engine OFF.
4. Use the scan tool to request the SIR DTC display.

Does the scan tool indicate that this DTC is current?

--

Go to Step 5

Go to Diagnostic Aids

5

1. Turn OFF the ignition.
2. Disconnect the 2-way inline connector.
3. Use the J 38715-90 adaptor to connect the J 38715-A SIR Driver/Passenger Load Tool BASE OF COLUMN connector to the female side of the inflatable restraint steering wheel module coil wiring harness connector.
4. Turn ON the ignition, with the engine OFF.
5. Use the scan tool to request the SIR DTC display.

Does the scan tool indicate that this DTC is current?

--

Go to Step 9

Go to Step 6

6

1. Turn OFF the ignition.
2. Disconnect the J 38715-A .
3. Reconnect the inline connector.
4. Disconnect the inflatable restraint steering wheel module. Refer to Inflatable Restraint Steering Wheel Module Replacement .
5. Use the J 38715-30A to connect the J 38715-A to the upper inflatable restraint steering wheel module coil connector.
6. Turn ON the ignition, with the engine OFF.
7. Use the scan tool to request the SIR DTC display.

Does the scan tool indicate that this DTC is current?

--

Go to Step 8

Go to Step 7

7

1. Turn OFF the ignition.
2. Replace the inflatable restraint steering wheel module. Refer to Inflatable Restraint Steering Wheel Module Replacement .

Did you complete the replacement?

--

Go to Step 16

--

8

1. Turn OFF the ignition.
2. Replace the inflatable restraint steering wheel module coil. Refer to Inflatable Restraint Steering Wheel Module Coil Replacement .

Did you complete the replacement?

--

Go to Step 16

--

9

1. Turn OFF the ignition.
2. Remove the J 38715-A .
3. Disconnect the inflatable restraint sensing and diagnostic module (SDM). Refer to Inflatable Restraint Sensing and Diagnostic Module Replacement .
4. Inspect the SDM wiring harness connector for the following conditions:

• | Corrosion

• | Damaged terminals

• | Poor connections/terminal tension

5. Refer to Testing for Intermittent Conditions and Poor Connections in Wiring Systems.

Does the SDM wiring harness connector exhibit any signs of corrosion, terminal damage, or poor connections?

--

Go to Step 10

Go to Step 11

10 | Replace the SDM wiring harness connector. Refer to Connector Repairs in Wiring Systems. Did you complete the repair? | -- | Go to Step 16 | --

11

1. Zero the J 39200 Digital Multimeter (DMM).
2. Use the DMM to measure the resistance of the driver high circuit.

Does the resistance measure less than the specified value?

0.5 ohms

Go to Step 13

Go to Step 12

12 | Locate and repair the open or the high resistance in the driver high circuit. Refer to Circuit Testing and Wiring Repairs in Wiring systems. Did you complete the repair? | -- | Go to Step 16 | --
13 | Use the DMM to measure the resistance of the driver low circuit. Does the resistance measure less than the specified value? | 0.5 ohms | Go to Step 15 | Go to Step 14
14 | Locate and repair the open or the high resistance in the driver low circuit. Refer to Circuit Testing and Wiring Repairs in Wiring systems. Did you complete the repair? | -- | Go to Step 16 | --
15 | Replace the SDM. Refer to Inflatable Restraint Sensing and Diagnostic Module Replacement . Did you complete the replacement? | -- | Go to Step 16 | --

16

1. Reconnect all SIR components.
2. Verify that all components and connectors are properly mounted.
3. Turn ON the ignition, with the engine OFF.
4. Use the scan tool in order to clear the DTCs.

Did you complete the action?

--

Go to Diagnostic System Check - SIR

--