Rear Floor Carpet Trim Plate Replacement. Buick GL7 (Export) 2000

For 1990-2009 cars

### Removal Procedure

1. Remove the rear seats. Refer to Rear Seat Replacement in Seats.
2. Remove the locking clips from the bezel using a curved pick tool.
3. Unsnap the anchor plate bezel (1) from the floor.

### Installation Procedure

1. Snap into place the anchor plate bezel (1) to the floor.
2. Snap into place the locking clips to the bezel.
3. Install the rear seats. Refer to Rear Seat Replacement in Seats.