Rear Bumper Fascia Reflector Replacement. Buick GL7 (Export) 2000

For 1990-2009 cars

### Removal Procedure

1. Use a heat gun in order to heat the rear bumper fascia appliques. Hold the heat gun 152 mm (6 in) from the surface.
2. Use a circular motion for 30 seconds when applying heat to the surface.
3. Use a flat-bladed tool in order to peel the rear bumper fascia appliques from the rear bumper fascia surface.

Do not damage the paint.

4. Use oil-free naphtha or alcohol in order to clean the rear bumper fascia.

### Installation Procedure

1. Warm the rear bumper fascia with a heat lamp or heat gun to a minimum of 21°C (70°F).
2. Peel the backing from the front end of the rear bumper fascia appliques.

Important: Do not touch the adhesive backing.

3. Press the rear bumper fascia appliques to the rear fascia while continuing to remove the backing.
4. Hand roll the rear bumper fascia appliques to the rear fascia in order to ensure proper adhesion.