Sliding Door Window Weatherstrip Replacement. Buick GL7 (Export) 2000

For 1990-2009 cars

### Removal Procedure

1. Remove the sliding door swing out window. Refer to Front Side Door Window Belt Inner Sealing Strip Replacement .
2. Pull the sliding door window weather-strip from the pinch-weld flange.
3. Remove the sliding door window weather-strip from the sliding door.

### Installation Procedure

Important: The swing out window weather-strip service replacement part is a cut-to-fit part. The weather-strip must be trimmed to fit the window opening and joined together.

1. Install the sliding door window weather-strip to the sliding door.
2. Align the sliding door window weather-strip to so the joint is at the center of the sliding door window latch attachment point.
3. Roll the sliding door window weather-strip from the joint to the bottom of the window in order to ensure a proper seal.
4. Install the sliding door swing out window. Refer to Front Side Door Window Belt Inner Sealing Strip Replacement .