EXHAUST RATTLE (SHIM EXHAUST HANGER). Buick Reatta 1989

For 1990-2009 cars

# EXHAUST RATTLE (SHIM EXHAUST HANGER)

#### VEHICLES AFFECTED: 1989 E

Some 1989 Buick Rivieras bulit before VIN 415557 may experience a condition of an exhaust rattle. This condition may be caused by the exhaust system contacting the underbody brace. To repair this condition shim the underbody brace 6 mm (1/4") from the underbody using two 3 mm (1/8") washers or equivalent at each bolt location. Refer to Figure 1.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.